**MUNICIPAL ROADS GRANTS-IN-AID PROGRAM**

**Final Performance Report**

**Project Information**

Municipality:

Report date:

Grants-in-Aid funding amount:

Total match documented (20% of total project(s) cost):

**Complete this table indicating road segments worked on and *linear practices* implemented along paved and gravel roads with ditches (e.g., stone-lined ditch, lowering of high road shoulder, etc.).**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Road segment ID # | Hydrologically connected? Yes/No | Road condition 1 before project implementation | Itemized practices implemented to improve road condition | Road condition 1  after project implementation | Date project constructed |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

1 – Road conditions are based on Municipal Roads General Permit (MRGP) standards. Please indicate one of the following three standards: (1) not meeting standards, (2) partially meeting standards, or (3) fully meeting standards.

**If your project involved outlet stabilization on paved roads with catch basins and/or Class 4 gully erosion remediation, complete this table.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Road segment or catch basin ID 2 | Hydrologically connected? Yes/No | Average estimated length of erosion | Average estimated width of erosion | Average estimated depth of erosion | Date project constructed |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

2 – Provide road segment ID for projects on Class 4 roads and catch basin ID for projects on paved roads with catch basins.

**Attach before and after photos for each road project completed, and photo of clean water project sign posted during construction (if applicable). Photos should be taken from the same perspective before and after project implementation and submitted as individual JPG files (minimum resolution 300 pixels per inch).**