|  |  |
| --- | --- |
| **Project Name:**  | **Discharge Point:**  |
| **Extreme Flood Protection Standard Waiver Worksheet** |
| Fill out this worksheet for each discharge point in which use of this waiver is sought. |
|  |
| **Extreme Flood Protection Standard (QP100) Waiver** (*check only one*)**:** |
| **[ ]**  | 1. A site that has a direct discharge to waters with a drainage area equal to or greater than or equal to 10 square miles and that is less than 5% of the watershed area at the site’s upstream boundary. |
| Name of Waters at Discharge Point: |  |
| Drainage Area of Waters at Discharge Point (square miles): |  |
|  [ ]  2. The impervious on site or otherwise associated within a common plan of development, constructed after 2002, is less than 10 acres.  [ ]  **Yes** **[ ]  No** |
|

|  |  |  |
| --- | --- | --- |
|  |  |  |
| **[ ]**  | 3. A downstream analysis was completed, pursuant to Section 2.5 of the 2017 VSMM, that indicated extreme flood control is not necessary for the site. |  |  |
| Has adequate conveyance from the site to the discharge point been verified? | **[ ]  Yes [ ]  No** |  |  |
| Has supporting information (e.g. narrative description, calculations, modeling) for the completed downstream analysis been included with the application? | **[ ]  Yes [ ]  No** |  |  |
|  |  |  |

*For a project that has more than one discharge point and that discharges to different receiving waters, waiver eligibility shall be determined on a “per receiving water” basis. Receiving waters are considered separate if the drainage area at their downstream point of confluence is greater than 10 square miles.* |
| *For example, if discharge point S/N 001 drains directly to the Winooski River (greater than 10 square miles), but discharge point S/N 002 drains to a small tributary of the Winooski River, then S/N 001 could be waived from the Extreme Flood Protection Treatment Standard using Waiver 2, but S/N 002 could not. However, S/N002 may be still eligible for Waiver 1.* |